|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| measuring cylinder |  | | retort stand, boss head and clamp | | |  |
| * Measuring accurate volumes of liquids | | | * Used to support equipment * The boss head holds the clamp to the retort stand | | | |
| Bunsen burner | WS0108_00883-r | | gauze mat | | |  |
| * Used for heating equipment or chemicals | | | * Placed on a tripod to spread heat evenly | | | |
| tripod |  | | evaporating basin | | | WS0111_00883-r |
| * Supports equipment over a Bunsen burner | | | * Evaporating liquids quickly over a Bunsen burner | | | |
| filter funnel | WS0113_00883-r | | conical flask | | | WS0114_00883-r |
| * Pouring liquids into narrow containers * Filtering solids out of liquids | | | * Holding large amounts of liquids * Heating liquids | | | |
| thermometer | WS0117_00883-r | | test tube rack | | | WS0119_00883-r |
| * Measuring temperature | | | * Holding test tubes | | | |
| spatula | | WS0120_00883-r | | heatproof mat |  | |
| * Picking up solids | | | | * Placed under equipment to protect the bench | | |
| watch glass | | WS0111_00883-r | | pipe clay triangle |  | |
| * Holding small specimens * Evaporating liquids quickly | | | | * Holding containers like evaporating basins over a Bunsen burner | | |